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CALIBRATION MACHINE WINTER SANDOMAT RP 1300, YEAR OF MANUFACTURE 2014 IN PERFECT WORKING CONDITION
Technical details:
- working width 1300 mm
- minimum piece length 535 mm
- thickness min./max. piece 2 / 160 mm
- forward speed without steps 3 - 30 m/min.
1. Grinding aggregate
- rubber contact roller with grooves 80 sh
- 22 kW / 400 V motor
- calibration roller Ø 240 mm
- sanding belt speed 20 m/s
2. Grinding aggregate
- aggregate combined with roller 70 sh / slipper
- 18.5 kW / 400 V motor
- roller contact rubber and with grooves Ø 210 mm
- operational command at input/output
- sanding belt speed 18 m/s
- Advance motor 4.0 kW
- Height adjustment motor 0.37 kW
- Total power 45 kW
- dimensions of the sanding belt 1330 x 2500 mm
- air pressure 8 bar
- air consumption 17 m3/h
- automatic centering of the advance carpet
- Digital display with automatic adjustment of working thickness
- CIGO rubber transport carpet
- Automatic star-delta start
- Pneumatic tensioning of the sanding belts
- Protective guards for the operator and for parts with automatic release
- Ammeter for controlling the grinding thickness
- Emergency button with automatic braking system
- Pneumatic cleaning of the sanding belt
- Cleaning brushes for cleaning
- CE standard, TÜV Rheinland
- Dimensions L=2095, l=2150, H=2200 mm
- Weight 3100 kg

PRICE 14500 EURO PLUS VAT
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